# Adjusting wheel guard

DANGER

Risk of Injury

There is a risk of injury if the tool is used without the wheel guard.

- Always use the tool with the recommended wheel guard.

- Make sure that the wheel guard is positioned correctly and not damaged.

WARNING

Risk of severe injury

Air under pressure can cause injury.

- Always shut off the air supply when not in use or before any adjustments.

- Drain the hose of air pressure and disconnect the tool from air supply when not in use or before any adjustments.

- Always use the correct hose size and air pressure for the tool.

Instructions

1. Pull and hold the spindle lock button.

2. Turn the wheel guard in a suitable position. Position the wheel guard between yourself and the grinding wheel.

   WARNING

   Risk of injury

   - Make sure that the wheel guard is put in a suitable position before operating the tool.

3. Release the spindle lock button. Make sure that the spindle lock pin snaps into place in one of the holes in the wheel guard.