# Operating the grinder

DANGER

Risk of Injury

There is a risk of injury if the tool is used without the wheel guard.

- Always use the tool with the recommended wheel guard.

- Make sure that the wheel guard is positioned correctly and not damaged.

WARNING

Risk of injury

- Always use applicable protective equipment when working with the tool such as; eye protection, hearing protection and non skid safety shoes.

- Always wear protective gloves when replacing accessories or when making repairs.

- Make sure that the working area is kept free from other people to prevent injuries.

- Make sure that the workpiece is safely attached.

- Make sure that the air hose is not under pressure before connecting the tool to the air supply.

- Never remove or attach the throttle lever or security mechanism with tape or similar.

- Make sure that the selected combination of abrasive equipment and attachments parts correspond to national regulations.

- Make sure that the abrasive equipment is not cracked or damaged.

- Make sure that the maximum speed of the abrasive equipment is higher than or equal to the speed marked on the tool.

- Make sure that the speed of the tool is not higher than the maximum rated speed marked on the tool.

- When working with the tool, always hold the tool with two hands and in such a way that they are kept away from moving parts.

- Always operate the tool in the recommended working direction.

- Never touch any rotating parts when the tool is running or connected to the air line.

- Never use the tool above head height.

- Stop using the tool if abnormally loud noises and vibrations occur during use.

Instructions

1. Connect the tool to the air supply (if not already connected).

   Direct the air exhaust away from the operator.

2. Press the release arm forward to release the security mechanism.

   Press down the throttle lever to start the tool.

WARNING

Risk of Damage and Injury

Rotating parts may cause damage and injury

- Make sure that the tool is switched off and has stopped rotating before putting it down.