# Adjusting support handle

WARNING

Risk of severe injury

Air under pressure can cause injury.

- Always shut off the air supply when not in use or before any adjustments.

- Drain the hose of air pressure and disconnect the tool from air supply when not in use or before any adjustments.

- Always use the correct hose size and air pressure for the tool.

Required tools:

- Allen key

Instructions

1. Loosen the support handle using an Allen key.

2. Adjust the support handle in a suitable position.

3. Tighten the support handle with the screw to 10 Nm (7.4 ft-lb).

   WARNING

   Risk of injury

   - Make sure that the wheel guard is put in a suitable position before operating the tool.