# Wheel configuration options

The table below shows the configuration options for different wheel types with applicable attachment parts.

For ordering number, see Spare Parts and Accessories in ServAid. For instructions on installing the wheel, see section Operating Instructions.

Pos. | Item | A. Grinding | B. Cutting-off
--- | --- | --- | ---
1 | Wheel | Type 27, Type 42 | Type 41
| Max diameter | 125 mm, 5" | 125 mm, 5"
| Thickness | 0.5–7.0 mm | 0.5–7.0 mm
| Hole diameter | 22 mm | 22 mm
| Peripherical speed | 80 m/s | 80 m/s
2 | Flange washer locking wheel | Ø 41 mm | Ø 58 mm
| Service tool | Allen key, 6 mm | Allen key, 6 mm
| Recommended torque | 20 Nm (14.8 ft-lb) | 20 Nm (14.8 ft-lb)