# Cleaning the adapter with strainer

WARNING

Risk of severe injury

Air under pressure can cause injury.

- Always shut off the air supply when not in use or before any adjustments.

- Drain the hose of air pressure and disconnect the tool from air supply when not in use or before any adjustments.

- Always use the correct hose size and air pressure for the tool.

Required tools:

- Vice

- Torque wrench

- Wrench (3/8")

- Blow gun

Spare parts:

- Replace the filter at every 1000-hour service.

Instructions

1. Position the tool in a vice.

   Disconnect the air adapter from the handle using a wrench.

2. Clean the adapter strainer using a blow gun.

   Replace the adapter with strainer if any damage or malfunction is detected.

3. Assemble the cleaned or new adapter with strainer with the o-ring.

   Fit the adapter with strainer in the handle and tighten using a wrench to recommended torque.