# Service interval overview

The table below shows the recommended service intervals for this tool, including what parts to service after 500, 1000, and 1500 working hours, and so on.

Every 1000 hours service must only be carried out by authorized workshop or qualified service technician.

500 hours service | 1000 hours service | 1500 hours service
--- | --- | ---
Inspect tool visually | Inspect tool visually | Inspect tool visually
Change oil | Change oil | Change oil
Clean filters | Clean filters | Clean filters
| Service turbine |
| Service spindle |

## Maintenance kits

500 hours service | 1000 hours service | 1500 hours service
--- | --- | ---
Oil tube kit | Oil tube kit × 2 | Oil tube kit
Maintenance kit - 500 h | Maintenance kit - 500 h | Maintenance kit - 500 h
| Maintenance kit - 1000 h |